### Group By XS Order(ascending)

XS DC 02 | Constant discharge used for the entire profile for 1%-annual-chance flood. At least two discharges should be selected; one at the mouth and the other at the middle of the watershed or above the confluence of a tributary. Or provide explanation why only one discharge should be used. Other flood frequencies should also be checked.
XS CD 01 | SECNO: 58
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS CD 01 | SECNO: 102
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS IF 01R | SECNO: 102
| Flow code will be IR. The area to the right of the ineffective flow station may be considered effective. The 1%-annual-chance WSEL of 2392 is higher than the ground elevation 2391.578 of the Right Ineffective Flow Station. However, it is equal to or lower than the right ineffective flow elevation of 2395.23. The lateral structure was not modeled downstream of this River Station. Lower the ineffective flow elevation to the ground elevation to consider the area right of the ineffective flow station as effective, or model a lateral structure if the overflow will take a different flow path. The ineffective flow elevation could be accepted if the area right of the ineffective flow station is non conveyance.
XS CD 01 | SECNO: 322
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS CD 01 | SECNO: 464
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS CD 01 | SECNO: 939
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS CD 01 | SECNO: 1480
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS CD 01 | SECNO: 1613
| Critical Depth occurs at 1%-annual-chance flood. Flow Code will be "C". The Ineffective flow option is used. The Ineffective Flow elevation is equal to or higher than the Critical WSEL. Please investigate whether this selection is appropriate.
XS IF 01R | SECNO: 1613
| Flow code will be IR. The area to the right of the ineffective flow station may be considered effective. The 1%-annual-chance WSEL of 2471.69 is higher than the ground elevation 2470.989 of the Right Ineffective Flow Station. However, it is equal to or lower than the right ineffective flow elevation of 2475.58. The lateral structure was not modeled downstream of this River Station. Lower the ineffective flow elevation to the ground elevation to consider the area right of the ineffective flow station as effective, or model a lateral structure if the overflow will take a different flow path. The ineffective flow elevation could be accepted if the area right of the ineffective flow station is non conveyance.