### XS Placement

XS DF 01R | SECNO: 290
| Divided flow. Flow code will be DR. The 1%-annual-chance flood discharge has a divided flow. The starting and ending stations of the cross section should not extend beyond the watershed boundary of the studied stream. Please review the extent of the cross section. If the cross section extends beyond the watershed boundary then the cross section needs to be trimmed and the HEC-RAS geometry file may need to be recreated using a GIS program. Or use the ineffective flow option, if it has not been considered, to limit the extent of the cross section or to block the divided flow area if it is a local depression.