Proj Title=PECKSRN
Current Plan=p01
Default Exp/Contr=0,0
English Units
Geom File=g01
Flow File=f01
Plan File=p01
Y Axis Title=
X Axis Title(PF)=
X Axis Title(XS)=
BEGIN DESCRIPTION:
---------- MODELED AS PART OF WVEMD CTP PROGRAM, 2023----------
Stream Name: Pecks Run
Flood Zone:  AFH
Upshur County, WV
 
HEC-RAS Version: RAS 6.3
Vertical Datum: NAVD88
Projection: NAD 1983 StatePlane West Virginia S FIPS 4702 (US Feet)
Terrain: 1-meter LIDAR (FEMA Region III 3DEP collected 2016-2018)
Land Use: 2019 NLCD

Hydrologic Method:
WV SIR2010-5033 regression equations

Additional Model Notes:
None

END DESCRIPTION:
DSS Start Date=
DSS Start Time=
DSS End Date=
DSS End Time=
DSS File=dss
DSS Export Filename=
DSS Export Rating Curves= 0 
DSS Export Rating Curve Sorted= 0 
DSS Export Volume Flow Curves= 0 
DXF Filename=
DXF OffsetX= 0 
DXF OffsetY= 0 
DXF ScaleX= 0 
DXF ScaleY= 0 
GIS Export Profiles= 0 
