BEGIN_USGS_DOQ_HEADER                                                         *
QUADRANGLE_NAME "LAVALETTE"                              3.45 or 7.5-min. name*
QUADRANT NE                     quadrant indicator if cell size = 3.75-minutes*
WEST_LONGITUDE -82 26 15.000                 signed deg min sec SDDD MM SS.SSS*
EAST_LONGITUDE -82 22 30.000                 signed deg min sec SDDD MM SS.SSS*
NORTH_LATITUDE 38 22 30.000                  signed deg min sec SDDD MM SS.SSS*
SOUTH_LATITUDE 38 18 45.000                  signed deg min sec SDDD MM SS.SSS*
PRODUCTION_DATE 2000  8 23                                          yyyy mm dd*
RASTER_ORDER left_right/top_bottom                         video display order*
BAND_ORGANIZATION BIP                        single file or BSQ, or BIL or BIP*
BAND_CONTENT RED                                 black&white or red green blue*
BAND_CONTENT GREEN                               black&white or red green blue*
BAND_CONTENT BLUE                                black&white or red green blue*
BITS_PER_PIXEL 8                                        radiometric resolution*
SAMPLES_AND_LINES 6190 7639                         number of columns and rows*
HORIZONTAL_DATUM NAD83                                primary horizontal datum*
HORIZONTAL_COORDINATE_SYSTEM UTM                                              *
COORDINATE_ZONE 17                               coordinate system zone number*
HORIZONTAL_UNITS meters                                coordinate system units*
HORIZONTAL_RESOLUTION 1.00                 pixel horiz. ground sample distance*
SECONDARY_HORIZONTAL_DATUM NAD27                    secondary horizontal datum*
XY_ORIGIN 374020.000 4248716.000         coord. of upper left pixel pri. datum*
SECONDARY_XY_ORIGIN 374005.832 4248500.370    coord upper left pixel sec datum*
NATION US                                                          nation code*
STATE WV                                                        state fip code*
NW_QUAD_CORNER_XY 374433.676 4248401.373     XY coords. of pri. NW quad corner*
NE_QUAD_CORNER_XY 379893.329 4248318.168     XY coords. of pri. NE quad corner*
SE_QUAD_CORNER_XY 379790.056 4241382.791     XY coords. of pri. SE quad corner*
SW_QUAD_CORNER_XY 374325.705 4241465.953     XY coords. of pri. SW quad corner*
SECONDARY_NW_QUAD_XY 374430.507 4248194.839     XY coords. - sec. NW quad cor.*
SECONDARY_NE_QUAD_XY 379890.299 4248111.632     XY coords. - sec. NE quad cor.*
SECONDARY_SE_QUAD_XY 379787.027 4241176.400     XY coords. - sec. SE quad cor.*
SECONDARY_SW_QUAD_XY 374322.539 4241259.564     XY coords. - sec. SW quad cor.*
RMSE_XY 1.22                                               doq horiz. accuracy*
IMAGE_SOURCE "COLOR INFRA-RED FILM"             b&w, cir, natural color, other*
SOURCE_IMAGE_ID "NAPP 9453-055"                                source image id*
SOURCE_IMAGE_DATE 1996  4  2                   source image date as yyyy mm dd*
SOURCE_DEM_DATE 1997  6  1                          source dem date yyyy mm dd*
AGENCY "WESTERN MAPPING CENTER (WMC)"                         oversight agency*
PRODUCER "WOOLPERT LLP"                                    producer/contractor*
PRODUCTION_SYSTEM "INTERGRAPH ISPM, ISIR"                    production system*
STANDARD_VERSION 1996 12                               version of DOQ standard*
METADATA_DATE 2000  8 23                   date created or changed, yyyy mm dd*
DATA_FILE_SIZE 141874800                                data set size in bytes*
BYTE_COUNT 18570                                             header byte count*
