BEGIN_USGS_DOQ_HEADER                                                         *
QUADRANGLE_NAME "MANNINGTON"                             3.45 or 7.5-min. name*
QUADRANT NE                     quadrant indicator if cell size = 3.75-minutes*
WEST_LONGITUDE -80 18 45.000                 signed deg min sec SDDD MM SS.SSS*
EAST_LONGITUDE -80 15  0.000                 signed deg min sec SDDD MM SS.SSS*
NORTH_LATITUDE 39 37 30.000                  signed deg min sec SDDD MM SS.SSS*
SOUTH_LATITUDE 39 33 45.000                  signed deg min sec SDDD MM SS.SSS*
PRODUCTION_DATE 1999 10 14                                          yyyy mm dd*
RASTER_ORDER left_right/top_bottom                         video display order*
BAND_ORGANIZATION BIP                        single file or BSQ, or BIL or BIP*
BAND_CONTENT RED                                 black&white or red green blue*
BAND_CONTENT GREEN                               black&white or red green blue*
BAND_CONTENT BLUE                                black&white or red green blue*
BITS_PER_PIXEL 8                                        radiometric resolution*
SAMPLES_AND_LINES 6050 7600                         number of columns and rows*
HORIZONTAL_DATUM NAD83                                primary horizontal datum*
HORIZONTAL_COORDINATE_SYSTEM UTM                                              *
COORDINATE_ZONE 17                               coordinate system zone number*
HORIZONTAL_UNITS meters                                coordinate system units*
HORIZONTAL_RESOLUTION 1.00                 pixel horiz. ground sample distance*
SECONDARY_HORIZONTAL_DATUM NAD27                    secondary horizontal datum*
XY_ORIGIN 558699.000 4386721.000         coord. of upper left pixel pri. datum*
SECONDARY_XY_ORIGIN 558683.530 4386502.536    coord upper left pixel sec datum*
NATION US                                                          nation code*
STATE WV                                                        state fip code*
NW_QUAD_CORNER_XY 559004.817 4386363.011     XY coords. of pri. NW quad corner*
NE_QUAD_CORNER_XY 564368.947 4386405.929     XY coords. of pri. NE quad corner*
SE_QUAD_CORNER_XY 564426.820 4379469.415     XY coords. of pri. SE quad corner*
SW_QUAD_CORNER_XY 559057.867 4379426.515     XY coords. of pri. SW quad corner*
SECONDARY_NW_QUAD_XY 559006.353 4386153.732     XY coords. - sec. NW quad cor.*
SECONDARY_NE_QUAD_XY 564370.622 4386196.651     XY coords. - sec. NE quad cor.*
SECONDARY_SE_QUAD_XY 564428.494 4379260.265     XY coords. - sec. SE quad cor.*
SECONDARY_SW_QUAD_XY 559059.402 4379217.364     XY coords. - sec. SW quad cor.*
RMSE_XY 2.40                                               doq horiz. accuracy*
IMAGE_SOURCE "COLOR INFRA-RED FILM"             b&w, cir, natural color, other*
SOURCE_IMAGE_ID "NAPP 9435-024"                                source image id*
SOURCE_IMAGE_DATE 1996  3 27                   source image date as yyyy mm dd*
SOURCE_DEM_DATE 1994  0  0                          source dem date yyyy mm dd*
AGENCY "WESTERN MAPPING CENTER (WMC)"                         oversight agency*
PRODUCER "WOOLPERT LLP"                                    producer/contractor*
PRODUCTION_SYSTEM "INTERGRAPH ISPM, ISIR"                    production system*
STANDARD_VERSION 1996 12                               version of DOQ standard*
METADATA_DATE 1999 10 14                   date created or changed, yyyy mm dd*
DATA_FILE_SIZE 137958150                                data set size in bytes*
BYTE_COUNT 18150                                             header byte count*
