BEGIN_USGS_DOQ_HEADER                                                         *
QUADRANGLE_NAME "PETERSTOWN"                             3.45 or 7.5-min. name*
QUADRANT SW                     quadrant indicator if cell size = 3.75-minutes*
WEST_LONGITUDE -80 52 30.000                 signed deg min sec SDDD MM SS.SSS*
EAST_LONGITUDE -80 48 45.000                 signed deg min sec SDDD MM SS.SSS*
NORTH_LATITUDE 37 26 15.000                  signed deg min sec SDDD MM SS.SSS*
SOUTH_LATITUDE 37 22 30.000                  signed deg min sec SDDD MM SS.SSS*
PRODUCTION_DATE 1999 10  1                                          yyyy mm dd*
RASTER_ORDER left_right/top_bottom                         video display order*
BAND_ORGANIZATION BIP                        single file or BSQ, or BIL or BIP*
BAND_CONTENT RED                                 black&white or red green blue*
BAND_CONTENT GREEN                               black&white or red green blue*
BAND_CONTENT BLUE                                black&white or red green blue*
BITS_PER_PIXEL 8                                        radiometric resolution*
SAMPLES_AND_LINES 6172 7568                         number of columns and rows*
HORIZONTAL_DATUM NAD83                                primary horizontal datum*
HORIZONTAL_COORDINATE_SYSTEM UTM                                              *
COORDINATE_ZONE 17                               coordinate system zone number*
HORIZONTAL_UNITS meters                                coordinate system units*
HORIZONTAL_RESOLUTION 1.00                 pixel horiz. ground sample distance*
SECONDARY_HORIZONTAL_DATUM NAD27                    secondary horizontal datum*
XY_ORIGIN 510752.000 4143743.000         coord. of upper left pixel pri. datum*
SECONDARY_XY_ORIGIN 510734.923 4143525.293    coord upper left pixel sec datum*
NATION US                                                          nation code*
STATE VA                                                        state fip code*
STATE WV                                                        state fip code*
NW_QUAD_CORNER_XY 511057.964 4143414.796     XY coords. of pri. NW quad corner*
NE_QUAD_CORNER_XY 516586.950 4143423.962     XY coords. of pri. NE quad corner*
SE_QUAD_CORNER_XY 516600.734 4136490.147     XY coords. of pri. SE quad corner*
SW_QUAD_CORNER_XY 511067.153 4136480.987     XY coords. of pri. SW quad corner*
SECONDARY_NW_QUAD_XY 511058.236 4143210.499     XY coords. - sec. NW quad cor.*
SECONDARY_NE_QUAD_XY 516587.359 4143219.665     XY coords. - sec. NE quad cor.*
SECONDARY_SE_QUAD_XY 516601.143 4136286.007     XY coords. - sec. SE quad cor.*
SECONDARY_SW_QUAD_XY 511067.425 4136276.847     XY coords. - sec. SW quad cor.*
RMSE_XY 2.54                                               doq horiz. accuracy*
IMAGE_SOURCE "COLOR INFRA-RED FILM"             b&w, cir, natural color, other*
SOURCE_IMAGE_ID "NAPP 9444-133"                                source image id*
SOURCE_IMAGE_DATE 1996  4  3                   source image date as yyyy mm dd*
SOURCE_DEM_DATE 1998  0  0                          source dem date yyyy mm dd*
AGENCY "WESTERN MAPPING CENTER (WMC)"                         oversight agency*
PRODUCER "WOOLPERT LLP"                                    producer/contractor*
PRODUCTION_SYSTEM "INTERGRAPH ISPM, ISIR"                    production system*
STANDARD_VERSION 1996 12                               version of DOQ standard*
METADATA_DATE 1999 10  1                   date created or changed, yyyy mm dd*
DATA_FILE_SIZE 140147604                                data set size in bytes*
