Input filename:  g:/img/wellsville se.img

Output filename: g:/mrsids/wellsville se.sid

Input filesize: 128.15 Mb (134,374,092 bytes)

Output filesize: 12.58 Mb (13,188,548 bytes)

Input BitRate: 8

Input Wordlength (in bits): 8

Target compression ratio: 10.00

Actual compression ratio: 10.19

File type: ERDAS Image

Georeferencing: Geo TIFF



Start time: Thu Dec 11 14:33:04 2008

Completion time: Thu Dec 11 14:33:45 2008

Intensity weight: 4.00

Gamma: 2.00

