BEGIN_USGS_DOQ_HEADER                                                         *
QUADRANGLE_NAME "CIRCLEVILLE"                            3.45 or 7.5-min. name*
QUADRANT NE                     quadrant indicator if cell size = 3.75-minutes*
WEST_LONGITUDE -79 26 15.000                 signed deg min sec SDDD MM SS.SSS*
EAST_LONGITUDE -79 22 30.000                 signed deg min sec SDDD MM SS.SSS*
NORTH_LATITUDE 38 45  0.000                  signed deg min sec SDDD MM SS.SSS*
SOUTH_LATITUDE 38 41 15.000                  signed deg min sec SDDD MM SS.SSS*
PRODUCTION_DATE 1999 12  3                                          yyyy mm dd*
RASTER_ORDER left_right/top_bottom                         video display order*
BAND_ORGANIZATION BIP                        single file or BSQ, or BIL or BIP*
BAND_CONTENT RED                                 black&white or red green blue*
BAND_CONTENT GREEN                               black&white or red green blue*
BAND_CONTENT BLUE                                black&white or red green blue*
BITS_PER_PIXEL 8                                        radiometric resolution*
SAMPLES_AND_LINES 6185 7654                         number of columns and rows*
HORIZONTAL_DATUM NAD83                                primary horizontal datum*
HORIZONTAL_COORDINATE_SYSTEM UTM                                              *
COORDINATE_ZONE 17                               coordinate system zone number*
HORIZONTAL_UNITS meters                                coordinate system units*
HORIZONTAL_RESOLUTION 1.00                 pixel horiz. ground sample distance*
SECONDARY_HORIZONTAL_DATUM NAD27                    secondary horizontal datum*
XY_ORIGIN 635473.000 4290606.000         coord. of upper left pixel pri. datum*
SECONDARY_XY_ORIGIN 635456.661 4290385.744    coord upper left pixel sec datum*
NATION US                                                          nation code*
STATE WV                                                        state fip code*
NW_QUAD_CORNER_XY 635778.126 4290193.397     XY coords. of pri. NW quad corner*
NE_QUAD_CORNER_XY 641209.563 4290287.987     XY coords. of pri. NE quad corner*
SE_QUAD_CORNER_XY 641332.642 4283352.017     XY coords. of pri. SE quad corner*
SW_QUAD_CORNER_XY 635896.467 4283257.473     XY coords. of pri. SW quad corner*
SECONDARY_NW_QUAD_XY 635781.585 4289986.015     XY coords. - sec. NW quad cor.*
SECONDARY_NE_QUAD_XY 641213.161 4290080.608     XY coords. - sec. NE quad cor.*
SECONDARY_SE_QUAD_XY 641336.236 4283144.778     XY coords. - sec. SE quad cor.*
SECONDARY_SW_QUAD_XY 635899.924 4283050.231     XY coords. - sec. SW quad cor.*
RMSE_XY 2.55                                               doq horiz. accuracy*
IMAGE_SOURCE "COLOR INFRA-RED FILM"             b&w, cir, natural color, other*
SOURCE_IMAGE_ID "NAPP 9434-023"                                source image id*
SOURCE_IMAGE_DATE 1997  4  8                   source image date as yyyy mm dd*
SOURCE_DEM_DATE 1998  0  0                          source dem date yyyy mm dd*
AGENCY "WESTERN MAPPING CENTER (WMC)"                         oversight agency*
PRODUCER "WOOLPERT LLP"                                    producer/contractor*
PRODUCTION_SYSTEM "INTERGRAPH ISPM, ISIR"                    production system*
STANDARD_VERSION 1996 12                               version of DOQ standard*
METADATA_DATE 1999 12  3                   date created or changed, yyyy mm dd*
DATA_FILE_SIZE 142038525                                data set size in bytes*
BYTE_COUNT 18555                                             header byte count*
