BEGIN_USGS_DOQ_HEADER                                                         *
QUADRANGLE_NAME "SANDYVILLE"                             3.45 or 7.5-min. name*
QUADRANT NE                     quadrant indicator if cell size = 3.75-minutes*
WEST_LONGITUDE -81 41 15.000                 signed deg min sec SDDD MM SS.SSS*
EAST_LONGITUDE -81 37 30.000                 signed deg min sec SDDD MM SS.SSS*
NORTH_LATITUDE 39 0  0.000                   signed deg min sec SDDD MM SS.SSS*
SOUTH_LATITUDE 38 56 15.000                  signed deg min sec SDDD MM SS.SSS*
PRODUCTION_DATE 2000  8 16                                          yyyy mm dd*
RASTER_ORDER left_right/top_bottom                         video display order*
BAND_ORGANIZATION BIP                        single file or BSQ, or BIL or BIP*
BAND_CONTENT RED                                 black&white or red green blue*
BAND_CONTENT GREEN                               black&white or red green blue*
BAND_CONTENT BLUE                                black&white or red green blue*
BITS_PER_PIXEL 8                                        radiometric resolution*
SAMPLES_AND_LINES 6089 7595                         number of columns and rows*
HORIZONTAL_DATUM NAD83                                primary horizontal datum*
HORIZONTAL_COORDINATE_SYSTEM UTM                                              *
COORDINATE_ZONE 17                               coordinate system zone number*
HORIZONTAL_UNITS meters                                coordinate system units*
HORIZONTAL_RESOLUTION 1.00                 pixel horiz. ground sample distance*
SECONDARY_HORIZONTAL_DATUM NAD27                    secondary horizontal datum*
XY_ORIGIN 440110.000 4317316.000         coord. of upper left pixel pri. datum*
SECONDARY_XY_ORIGIN 440095.510 4317099.252    coord upper left pixel sec datum*
NATION US                                                          nation code*
STATE WV                                                        state fip code*
NW_QUAD_CORNER_XY 440467.869 4317001.362     XY coords. of pri. NW quad corner*
NE_QUAD_CORNER_XY 445879.928 4316962.350     XY coords. of pri. NE quad corner*
SE_QUAD_CORNER_XY 445832.346 4310026.607     XY coords. of pri. SE quad corner*
SW_QUAD_CORNER_XY 440415.528 4310065.601     XY coords. of pri. SW quad corner*
SECONDARY_NW_QUAD_XY 440466.343 4316793.404     XY coords. - sec. NW quad cor.*
SECONDARY_NE_QUAD_XY 445878.541 4316754.391     XY coords. - sec. NE quad cor.*
SECONDARY_SE_QUAD_XY 445830.960 4309818.786     XY coords. - sec. SE quad cor.*
SECONDARY_SW_QUAD_XY 440414.003 4309857.781     XY coords. - sec. SW quad cor.*
RMSE_XY 1.24                                               doq horiz. accuracy*
IMAGE_SOURCE "COLOR INFRA-RED FILM"             b&w, cir, natural color, other*
SOURCE_IMAGE_ID "NAPP 9456-110"                                source image id*
SOURCE_IMAGE_DATE 1996  4 11                   source image date as yyyy mm dd*
SOURCE_DEM_DATE 1996  5  1                          source dem date yyyy mm dd*
AGENCY "WESTERN MAPPING CENTER (WMC)"                         oversight agency*
PRODUCER "WOOLPERT LLP"                                    producer/contractor*
PRODUCTION_SYSTEM "INTERGRAPH ISPM, ISIR"                    production system*
STANDARD_VERSION 1996 12                               version of DOQ standard*
METADATA_DATE 2000  8 16                   date created or changed, yyyy mm dd*
DATA_FILE_SIZE 138756132                                data set size in bytes*
BYTE_COUNT 18267                                             header byte count*
